Welcome to use the 24-Pin printers of our company!


The steps of installing the driver in the Windows 2000 or the Windows XP,Windows vista,Windows7:
*********************************************************
1. Please connect your printer to your computer with a interface cable, and then power on your printer.

2. Double click the named "setup.exe" program in the folder of "\WIN2000(XP-Vista-Win7)" in the driver disk.

3. Select the printer in the "Select Printer Driver" window and click the "Install" button. 
   
4. If a "Hardware Installation" window pops up, select "Continue Anyway".

5. Click the Exit button after installation successful.


Installing the driver in Windows 98 or Windows Me:
*********************************************************
1. In Start Menu Click "start"-->"settings"-->"Printers".

2. In Printers Manager Folder double click "Add Printer"-->"NEXT".

3. Click "NEXT" in the "Local or Network Printer", in which the default value is "Local Printer".

4. In the selection of "Manufacturers/Printers", click "Have Disk...", click "Browse".
   Choose the INF file in your printer driver disk, and continusly click "OK", and then click "NEXT". 
   
5. Select the print port you want to use in the "Available ports:" list.
      The default value is "LPT1: (Recommended Printer Port)", then click "NEXT".
      
6. You can type a name for your printer in the "Printer name:" textbox.
   And you can select to use this printer as the default printer.  
   And then click "Yes".
      
7. You can choose the "Yes" button in the "Print a test page" window if you'll like to test your printer(connect your printer to your computer with a interface cable and then turn on your printer).
  And then click "Finsh". the printer driver will be installed to your computer.

     (If a "Hardware Installation" window pops up, select "Continue Anyway".)

