| # Paper QSL Settings

Preferences–>QSL

You can’t change the layout of the printed label, but you can customize few lines. Currently following sizes are supported:

- Avery 3474 (37 mm x 70 mm at DIN A4, 3 x 8)
- Avery 3475 (36 mm x 70 mm at DIN A4 3 x 8)
- Avery 3653 (42.4 mm x 105 mm at DIN A4 2 x 7)
- Avery 4781 (42.3 mm x 97.0 mm at DIN A4, 2 x 6)
- Avery 5160 (1" x 2-5/8" at US-Letter 3 x 10)
- Avery 5161 (1" x 4" at US-Letter, 2 x 10)
- Avery 5163 (2" x 4" at US-Letter 2 x 5)
- Avery 7159 (34 mm x 64 mm at DIN A4, 3 x 8)
- Avery 7163 (38.1 mm x 99.1 mm at DIN A4 2 x 7)
- Avery 8162 (33.9 mm x 99.1 mm at DIN A4, 2 x 8)
- Avery 8462 (1-1/3" x 4" at US-Letter 2 x 7)
- Dymo 32 mm x 57 mm
- Dymo 89 mm x 36 mm
- Dymo 90 mm x 29 mm
- Dymo 1" x 2-1/8"
- Dymo 2-1/8 x 4"

The lower row can be printed per band, for example for the used equipment. When there is no text for a given band, the Default text will be used.
Not all rows will be printed to all label sizes!

You can set the text alignment per row, except the for the QSO data. These rows are always centered.

If you want to use another label size, e-mail me please.