| # In the Contest

### Important

- Enter the callsign of the current operator into the contest window.
- The QSO table can be adjusted, resorted and reordered by clicking into the headers.
- Use the space bar to toggle between Callsign and Rx Number field.
- S&P (Search and Pounce) will be activated as soon as you move the VFO.
- Enter the time intervall for Auto CW in the Preferences.
- Enter a frequency (kHz) into the callsign field to set the TRX (incl. mode)
- Enter a - into the callsign field to switch split on

### Callsign entry

While typing the log will be checked for new multipliers (if applicable)

#### CW Type Ahead

While sending CW, you can edit the callsign as long the character to edit was not sent yet! If you type slowly, you could enter just the prefix, start the exchange and while sending the prefix you can enter the suffix.

#### CW Correct function

The macro CORRECT can be used in the CW memories. When the callsign was edited after the exchange was sent, the corrected callsign will be given, otherwise nothing.
This is useful in the TU (F3) messaqe: CORRECT tu MY CALL test

#### Super Check Partial

The SCP runs while typing. All callsigns including the same character combination will be listed. The example on the left hand side shows the result after typing DL2R. Callsigns written in Red color are already in the log in this mode on this band (dupe). Callsigns written in Green color are in the log, but on another band or in another mode. Black colored callsigns are from the SCP database. They may be listed twice, if already in the log.

#### Similar Call Check

If you have ended the callsign entry, the Similar Call Check will be performed. This uses the SCP database only. Callsigns with another character on one position will be listed. This can help, when you have heard one character wrong. The example shows the result after entering DL2RUM.

### One QSO

#### The Enter key and the Return key

There are two Enter/Return keys on your keyboard. When you use a full keyboard, the Enter key is located on the right hand side in the numbers section. The Return key is located in keyboard main section.
On a Macbook keyboard is just the Return key direct accesable. To hit the Enter key, you have to press and hold the FN key as well.

When using these both keys, the results are slightly different and may have an effect of your work flow: When you press the Enter key, the QSO will be saved, but the TU message will not be sent! This is useful, when you made the QSO partly with a separate CW keyer.

#### General QSO

After entering the callsign, use the Space Bar to move the curser into the Received Number field. When the received number don’t require a Space, you can press the space bar again to go back to the callsign field.
Press the Enter or Return key to save the QSO.

ESM is available for all operating modes!

#### CW QSO without ESM

In the CW Preferences you have to define a key to start the exchange message (running station). When pressing this key, the callsign (type ahead) and the Exchange message (F2) will be sent.
Hitting the Return key saves the QSO and sends the TU message, while pressing the Enter key, the QSO will be saved only.

#### CW QSO using ESM

When you use a K1EL Winkey based CW keyer (or a microHAM device), make sure you have enabled the „Serial Echoback“ option in the RUMlogNG Preferences under the CW tab. RUMlog needs a feedback, which character is currently sent for the type ahead feature.
While in WSM mode the default button shows you the expected action pending on your current configuration:

- ESM Mode: Running or S&P
- Active entry field
- Content of an entry field

You can always use the CW memories (F1-F8) pending on the situation while in ESM

#### Running Station

#### Search & Pounce

### Statistics

See the Contest menu to open several statistic tables. Few tables are updated in real time, these are marked in the window title.
You can adjust the table columns as usually.