| # microHAM Devices

Preferences–>microHAM

microHAM devices may have very specific options, see the original documentation for use. You can use and configure the DKII and the MKII nearly to 100%, so the Windows Router software is not required any longer.

Use the settings in Preferences–>microHAM. The upper part is RUMlog specific, while the lower part is used within the microHAM device CAT control port. These info will be used and written to the device, as soon you use the CAT from RUMlog.

#### microKeyerII and DigiKeyerII

There is a small control window provided while using the DKII or MKII: Menu–>Window–>microHAM. Following functions are available:

- Keyer mode switching, pending on your settings (Voice MKII only)
- play back CW or RTTY memories
- abort memory playback
- shows status information, if window is extended
- further configurations

If the window has the focus, following shortcuts are available:

- C: CW Mode
- V: Voice Mode (MKII only)
- F: FSK Mode
- D: Digital Mode
- 1-9 memory playback
- Escape: abort playback

#### MKII und DKII Settings

It is important to understand, that the settings can’t be read from the device! All seen settings are saved on the computer to show it here. All settings can be stored permanently, or temporally until the next power reset. CW and RTTY memories are saved permanently always.

DKII Settings

MKII Settings

Edit CW Memories

# See Also

CAT Settings

K1EL WinKeyer

# External Links

microHAM