| # K3/KX2/KX3 Control

Menü–>Transceiver–>K3/KX2/KX3 Control

To use these advanced features, you have to select an Elecraft K3-Ctrl or KX3-Ctrl. There are minor differences between the K3 and the KX3 window.

#### Quick memories

In the upper right hand corner, you can find the table for quick memories. Pressing the + button saves a set of currently used frequency, mode, filter, RIT, XIT and split information. Double click a row to send these data back to the transceiver. The data are not editable.

#### Shortcuts

There are some functions with a shortcut. These are usable, when the window has the focus.

- 1 - 8 –> upper row of the macro buttons
- cmd 1 - cmd 8 –> lower row of the macro buttons
- F1 - F6 –> play memory 1-6 (KX3) or memory 1-4 & switch bank1/2 (K3)
- Escape –> abort transmission
- Enter –> direct frequency input

#### Direct Frequency Input

Just press the Enter key to tune VFO A, VFO B or set the split:

- VFO A: positive number in kHz > 100
  - 14195: VFO A tunes to 14195 kHz
- VFO B: negative number in kHz < -100
  - -21007,7: VFO B tunes to 21007,7 kHz
- Split: in kHz -100 bis +100
  - 2: VFO B equals VFO A and is incremented by 2 kHz

#### Macros

Use the button Edit to enter a macro button title or to edit the macros. There are 4 additional macros provided, started automatically after a mode change.

#### Panadapter

Menu–>Transceiver–>P3/PX3 Control

For the panadapter can be opened a separate control window. You can change settings, download a screen shot and the marker can be set using the mouse. Buttons are provided to duplicate the functions of the front panel FN keys. The keyboard keys 1-8 act as short cuts for the FN keys.

# External Links

K3 and KX3 Programmer's Reference