| # Station Info Box

Different error and status information will be written just above the box.
The information in the box is similar to the DXCC Info Box. A magenta written callsign indicates an invalid operation. Accurate sunset and sunrise times and bearing and distance information are available only, when the correct location is given in the Locator field.
To indicate a LoTW or eQSL AG member, you have to load the user lists first in: Menu–>Online.
A mouse click into the box brings up all QSOs with this station in the logbook table.