| # History

#### 1.0.3 04-February-2015

- First public version

#### 1.0.4 06-February-2015

- Fixed: Continent is updated now correctly in: Menu–>Logbook–>Recalculate DXCCs - Tnx W0DJC
- Fixed: Problem during HamQTH.com query after changes at the server site, Tnx OK2CQR

#### 1.0.5 20-February-2015

- Fixed: Crash when viewing an empty dx-spot database - Tnx DH2PAF
- Fixed: Time intervall for dx spot database queries was always fixed to e weeks, regardless of selection
- New: Label size Avery 3474 added for QSL label printing
- New: Better LoTW preferences, RUMlog reads now used callsigns and station locations from the tqsl settings
- New: ADIF tag OPERATOR added as export/import option for user defined fields
- New: P3 Control window: Menu–>Transceiver–>P3/PX3 control Use P3 Firmware >= 1.35

#### 1.0.6 21-February-2015

- Fixed: CAT for Kenwood is working again - Tnx DH6YMC and N1JM
- Fixed: rst will be set now according TRX mode - Tnx DH6YMC
- New: 33cm band added
- New: Table for supported bands/frequencies added under: Preferences–>QRGs

#### 1.0.7 26-February-2015

- Fixed: HamQTH.com shows now correct US State and County
- New: Label size Avery 4781 added for QSL label printing
- New: Text alignment options added for QSL label print out

#### 1.0.8 7-March-2015

If you are a LoTW user, you have to enter the path to the .tqsl folder! See the Lotw preferences.

- Fixed: qrz.com shows now the “addr1” information as well - Tnx DF4WA
- Fixed: CAT control will be disabled now before falling into sleep, this prevents problems after wake up in some configurations
- Fixed: Edited QSOs are shown now correct - Tnx KK6FNK
- Fixed: Text alignment on QSL label is affected now correct by settings - Tnx KK6FNK
- New: Label size Avery 5163 added for QSL label printing
- New: A click in a QSO row in the LoTW or eQSL In Window shows now all QSOs with this station in the Logging Window

#### 1.0.9 11-March-2015

- Fixed Better compatibility for 10.9, was not fixed in 1.0.8 - Tnx K4ZRJ & AL7EK
- Fixed: Statistics are corrected now for “invalid operation” All invalids count now. Recalculate your statistics to update: Menu–>Logbook–>Recalculate DXCCs Use the search options and select the invalids first. - Tnx NF4L
- New: You can choose now you own text- and background colors for dx spots in Preferences–>DX Alarm–>Set colors

#### 1.1 26-March-2015

Please check your settings in Preferences–>DX Alarm! There are major changes.

- Fixed: KX3 don’t send a @ in CW after pressing the Escape key - Tnx DK5LP
- Fixed: Better DXCC recognition for portable Operationen for 3B, EA, HC, TI, UA, ZL and ZS - Tnx LA0FA
- Fixed: LoTW Upload with satellietes QSOs corrected - Tnx EA2CQ
- Fixed: qrz.com shows all station images correct now - Tnx W0DJC
- New: DX Spots for New Ones can be spoken now - See also Preferences–>DX Alarm
- New: The opening of an extra spot window for searched stations is optional now
- New: Support for FTdx3000 - Tnx N2TSQ
- New: Support for FTdx5000 - Tnx LA0FA
- New: More AppleScript support for JT-Bridge - Tnx SM0THU
- New: A click into the bandmap on the call sign printout sets the TRX and the logging fields now
- New: You can take over data from previous QSOs during logging, see Preferences–>Databases for settings and the link “QSO Entry fields”
- New: A “No zoom” option added in the large map window, this prevents the map to zoom in automatically.
- New: Use of OS-X Notification Centre, use the System Preferences for further settings
- New: Toggle option: Menu–>Logbook–>Clear after QSY: clears all fields, when the VFO is tuned 1 kHz away
- New: More edit options when editing multiple QSOs with the same station
- New: DX spot window will be filled with data after “show/dx” as well
- New: All times are in 24 hours format now, regardless of system settings

#### 1.2 17-May-2015

- Fixed: DXCC computation for KG4 optimized - Tnx N1HO
- Fixed: IOTA reference for Oceania can now be entered correct - Tnx IK2EAE
- New: All areas currently located in the gray line can be listed in a separate table - See the link Miscellaneous Windows
- New: Support for Dymo Labelwriter format 57mm x 32mm - Tnx DL7XT
- New: Extended QSO search - See the link Miscellaneous Windows
- New: Support for FT-991 - Tnx DL4ABB
- New: Support for FTdx1200
- New: Dx Entity column added in the dx-spot tables
- New: Open unlimited number of band maps: Menu–>Window–>New Band Map
- New: Better CW window

#### 1.2.1 18-May-2015

- Fixed: CAT optimization for TS-2000 - Tnx WK8A

#### 1.2.2 20-May-2015

- Fixed: Preferences for user defined fields - Tnx DL2RUM

#### 1.2.3 23-May-2015

- Fixed: Zones are shown now correct after double clicking a dx-spot - Tnx IK2EAE

#### 1.2.4 13-June-2015

- Fixed: CW window Info field are not any longer mirrored in the rst field - Tnx DH6YMC
- Fixed: OS X notifications take eQSL and LoTW users now into consideration - Tnx NY4I

#### 1.2.5 3-July-2015

- Fixed: Printed QSL label shows correct rst now - Tnx OE1HXS
- Fixed: QSO Search window will be updated after log changes - Tnx DK5LP
- New: Support for FT-1000MP Mark-V - Tnx OE3ASA
- New: qrz.com/HamQTH.com informationen can be shown now below the logging window

#### 1.2.6 13-July-2015

- Fixed: problems with Timeout errors during up- and download fixed
- Fixed: Graphical issues fixed at the top of the band map
- Fixed: Data take over by a click into a band map works more reliable now
- New: DX-spot colors will be updated now after logging or deleting a QSO
- New: Option added to define the table columns width behavior while resizing the table: Preferences–>General–>Logbook behavior

#### 2.0 1-October-2015

- Fixed: Extended QSO Search will take the QSO time now into consideration - this was undefined before and the results unexpected - Tnx N8XMS
- New: Contest and dx-ped module
- New: Support for a second transceiver
- New: Support for Ten Tec Orion - Tnx ON5YA
- New: Support for QSL label Avery 5161 (US-Letter, 1" x 4" , 2 x 10)
- New: ADIF tag STATION_CALLSIGN added for im- and export of user fields

#### 2.1 24-October-2015

- Fixed: Window Calculations - When the date is changed, the sun times for location B will be recalculated now - Tnx DL2RUM
- Fixed: Contestlog: Scoring corrected, due to an error in saving the correct dxcc entity
- Fixed: Scoring for WWDX corrected - Tnx K6LE
- New: Support for label Avery 3653 (42.4mm x 105mm at DIN A4 2 x 7)
- New: In the Terminal window you can connect now up to 4 dx-cluster
- New: QSOs can be color coded in the log tables - Tnx M0CLH
- New: Ukrainian DX Contest

#### 2.2 3-November-2015

- Fixed: Textlabels show correct text color now
- Fixed: Bug during CAT initialization removed - Tnx DG3YJB
- New: QSO table background color can be given now during logging
- New: Apple Script support for Paper QSL
- New: A new drawer window in the contest interface can show all possible control numbers (multipliers) - if applicable
- New: JA DX Contest
- New: OK/OM DX Contest
- New: ARRL 160m Contest
- New: ARRL 10m Contest
- New: LZ DX Contest
- New: DARC XMAS Contest
- New: Croatian CW Contest

#### 2.3 27-November-2015

- Fixed: No more crashes when receiving specific LoTW QSLs - Tnx DL7VDX
- New: CQ zone (WAZ) can be set as dx alarm
- New: ADIF tag TIME_ON added for user definable logging fields
- New: Direct sql QSO search for experts in the QSO Search Window
- New: Support for Avery 8162 (DIN A4, 99.1 x 33.9 mm, 2 x 8)
- New: RTTY Operation in the Contest Modul via Fldigi or K3/KX3 (Contest und DX-Pedition)
- New: DARC Corona Contest
- New: OK RTTY DX Contest
- New: Ten-Meter RTTY Contest
- New: USKA XMAS Contest
- New: USKA Helvetia Contest
- New: General Contest (no scoring)

#### 2.4 13-December-2015

- Fixed: Crash during Cabrillo output when using OS-X 10.9 - Tnx OE1HXS
- New: You can add data from HamQTH.com or qrz.com to logbook entries: Menu–>QSO–>Add QSO data
- New: All band tables in the dx-spot window include now a contextual menu in the header to show/hide columns
- New: Search Entities Window: Select one or multiple Entities in the result table to mark appropriate QSOs - Tnx EA5FY
- New: Print QSL label: As alternate, you can select the last free label for the first sheet to print - Tnx SQ2KLU
- New: Dymo Label 57mm x 32mm now optional with one QSO and two footer rows
- New: DARC 10m Contest
- New: North American QSO Party
- New: REF Contest
- New: Brandenburg-Berlin Contest
- New: CQWW 160m Contest
- New: UBA DX Contest

#### 2.5 20-January-2016

- Fixed: QSL Manager was missing in Global QSL ADIF file - Tnx DK5CM
- New: More CW options in the Log Preferences under the CW tab - you have to reset your settings
- New: “New one” dx-spots can be notified using Growl
- New: You can remove now a callsign from a band map using cmd mouse click
- New: Separate band map and dx spot windows for the contest module
- New: Memory pad for contest operation
- New: Audio recording and play back functions
- New: QSO Export funktion for SOTA database (version 2)
- New: Support for Avery 7163
- New: Introduction of a Contest Cheat database - Tnx DL6ER
- New: AppleScript support for read/write of State, QSO date & time, the four user fields and for the Use real time checkbox
- New: ARRL Int. DX Contest
- New: CQ WPX contests - CW/SSB/RTTY
- New: PACC Contest

#### 2.5.2 31-January-2016

- Fixed: No more crashes when using some brands of external sound cards - Tnx EA5CQ, NA4M
- Fixed: Failure fixed, where the Preferences Window was completely unresposible - Tnx EA5CQ, NA4M
- Fixed: Ivory Coast (TU) is back on the DXCC list - Tnx IT9CML

#### 2.5.3. 17-February-2016

- Fixed: 10.9 (Mavericks) users can edit QSOs now again - Tnx AA4GA
- Fixed: QSOs for SOTA export are sorted now by date and time - Tnx W6UB
- Fixed: Cabrillo file shows now the correct frequency, after editing the band - Tnx Bill, AE6JV
- Fixed: Camden County, NJ added to database - Tnx IT9CML
- New: Dymo Label 89mm x 36mm

#### 2.6 3-March-2016

- Fixed: Interface problem band map/dx spot and contest window fixed - Tnx BG5EEF & K6LE
- New: DX spot window can show now the State (W), Province (VE) or the DOK (DL). A dx alarm can be set. You have to load the database first: Menu–>Online–>Load contest cheat database
- New: Elecraft P3 window shows now controls to change the P3 display font size and to toggle the TX meters. P3 Firmware MCU 01.57 oder newer required.
- New: Russian DX Contest
- New: RSGB Commonwealth Contest
- New: DARC Oster Contest
- New: South America 10m Contest

#### 2.7 29-March-2016

- Fixed: US-State now shown correctly in the 6m dx-spot table - Tnx IK2EAE
- New: Support for Avery 7159
- New: Dymo label 1" x 2-1/8"
- New: Dymo label 2-1/8 x 4"
- New: For the incoming eQSL you can define now the time slot for QSO-QSL time matching in the Preferences under the LoTW/eQSL tab.
- New: UBA ON Contest
- New: UBA Spring Contest
- New: SPDX Contest
- New: CWops Contest -> reload the Contest Cheat Database from the Online menu
- New: YU DX Contest
- New: Yuri Gagarin Contest
- New: Worked All Provinces of China DX Contest

#### 2.8 30-April-2016

- Fixed: ADIF Import: Deprecated Enumeration ‘V’ for the tags LOTW_QSL_RCVD und QSL_RCVD are interpreted as ‘Y’ now - Tnx K3DCW
- Fixed: Correction in the WPX prefix calculation - Tnx IV3TMM
- New: Changes for newest microHAM Firmware (3.3 for DKII and 6.3 for MKII)
- New: 7th Call Area QSO Party
- New: CQ-M International DX Contest
- New: A.R.I. International DX Contest
- New: His Majesty The King of Spain Contest
- New: Hessen Contest
- New: Hamburg Contest

#### 2.9 27-May-2016

- Fixed: Contest logging was impossible, when there is an apostrophe in the Computer’s name - Tnx G4AWP
- Fixed: DX-Cluster Auto Connect works now in the first terminal tab as expected - Tnx IV4TMM
- Fixed: Main Logging Window: Recently added or deleted QSOs are shown now correct in the Search section - Tnx IV4TMM
- Fixed: Data take over from previous QSOs: The newest datas will be used now - settings are saved now correct - Tnx IV4TMM
- New: Elecraft KX2 support added, including full control window
- New: In a log table selected QSO or the results from a DXCC entity search can be presented on a map - See the QSO menu
- New: IARU Region 1 Fieldday
- New: RSGB CW National Field Day
- New: Worked All VK Shires
- New: Portugal Day Contest
- New: World Wide South America CW Contest
- New: All Asian DX Contest (CW & SSB)
- New: Ukrainian DX Digi Contest

#### 2.10 26-June-2016

- Change: The Fldigi preferences can be found now under the µHAM/Fldigi tab, no changes in function
- New: Support for QSL label Avery 8462 (1-1/3" x 4" at US-Letter 2 x 7)
- New: IC-7300 control window - select IC-7300 Ctrl as transceiver
- New: The eight CW memories for the IC-7300 can be edited –> Menu–>Transceiver–>Edit CW memory
- New: You can set the serial CAT port flow control lines to High, to power up the interface
- New: Option added to use a Bluetooth Low Energy Modul CAT interface
- New: Provisions made to use the internal CW keyers in IC-7100, 7300, 7410, 7700, 7850, 7851 and 9100
- New: DXCC search: option added to search for exclusively LoTW or paper confirmed entities
- New: Command added to set the Paper QSO Status for selected QSOs to -: Menu–>QSL–>Do not send QSL. This works in the Search Windows as well.
- New: RAC Canada Day Contest
- New: Venezuelan Independence Contest
- New: DL-DX RTTY Contest
- New: IARU HF Championship
- New: RSGB Low Power Contest
- New: RSGB IOTA Contest

#### 2.10.1 28-June-2016

- Fixed: Connection to Fldigi controls in the Preferences repaired
- New: User fields can be mapped now to ADIF tags “MY_SIG” and “MY_SIG_INFO” (Used for WWFF)

#### 2.11 22-July-2016

- Fixed: RUMlog toggles PTT for Fldigi, while Fldigi in in Tune mode - Tnx Jwahar, KC1CCR
- New: Callsign auto complete function in the Paper QSL In window
- New: In the separate Map window, you can add a grid square overlay
- New: In HamQTH.com or qrz.com found postal addresses can be used for address label printing - See Menu–>QSL
- New: Satellite list updated
- New: For the grid square you can save now up to 10 digits
- New: The local time zone can be used instead of utc, see Preferences–>General–>Logbook behavior
- New: QSO Note field can be prefilled with data from a previous QSO: Preferences–>Databases–>Fill entry fields with data from previous QSOs
- New: European HF Championship
- New: RDA Contest
- New: YO DX HF Contest
- New: KCJ Contest
- New: WAEDC CW/SSB/RTTY - including QTC traffic

#### 2.12 25-August-2016

- Fixed: The window Receive Paper QSLs shows the QSOs with the selected colour code now - Tnx Terry, M0CLH
- Fixed: Entry of a / for a received QTC is possible now - Tnx DL1RF
- New: Load, view and save eQSL images Menu–>QSL–>Load eQSL image
- New: Apple Script support for the contest interface
- New: Use the internal CW keyer in the TS-480 - Tnx DL7VDX
- New: IC-7300 Control Window: Scope reference level can be saved and restored by band (optional)
- New: IC-7300 Control Window: Scope fixed edges can be selected matching the actual frequency (optional)
- New: Open a Contest or Logbook file by double click it or drop a file over the application icon
- New: Support for label printer format 90mm x 29mm
- New: If the option Menu–>Logbook–>Show prev. QSOs selected, the logbook will not show any longer an empty table when the station isn’t in the log yet
- New: CAT support for FT-840
- New: RSGB SSB Field Day
- New: FOC QSO Party (Please reload the Contest Cheat Database: Menu–>Online–>Load contest cheat Database)
- New: Africa All Mode International DX Contest
- New: New England QSO Party

#### 2.13 25-September-2016

- Fixed: General Contest: Failure in creating the serial number fixed - Tnx DK1OM
- New: Option added for Fldigi PTT switching
- New: Commands added to save all downloaded eQSL images and to close all windows - See Menu–>QSL
- New: QSOs can be deleted now from the Search QSOs window
- New: IC-7300 Control: Auto Hold Funktion for the Scope Center Mode
- New: qrz.com queries ignore /P, /M, /AM, /MM and /QRP
- Neu: Option added to reduce the number of grid square digits in the log after a HamQTH.com or qrz.com query: Preferences–>Databases
- Oceania DX Contest
- Pennsylvania QSO Party
- Russian World Wide Digital Contest
- California QSO Party
- RSGB International DX Contest
- Deutscher Telegraphie-Contest
- UK/EI DX Contest
- The Makrothen Contest
- JARTS WW RTTY CONTEST
- CQ WW DX Contest RTTY

# See Also

Options for PTT switching

Load eQSL Images

# External Links