| # Transceiver Control

The list of supported transceivers is quite short right now. When you are able to help out with another model, please contact me.
Fldigi has an own CAT control, RUMlog can control a TRX through Fldigi. Pending on the specific model, you have the following possibilities:

- exchange of frequency and mode
- switching PTT for Fldigi
- use of trx internal cw memories
- use of internal CW keyer
- CW speed setting

In most cases VFO A is controlled. There are advanced features provided for the IC-7300, Elecraft K3, KX2 and KX3.

#### Transceiver –> RUMlog

Frequency and operation mode will be written into the logging fields. Overriding the mode is possible with the deactivated option Follow TRX. This may be useful for digital modes. The frequency is used in the band map as well: Menu–>Window–>Band Map

#### RUMlog –> Transceiver

Here are the ways to tune the trx:

- enter a frequency (in kHz) into the callsign entry field followed by an Enter
- double click in the Frequency column in the dx spot or dx station alarm window
- click in the band map

The mode follows always the frequency defined in Preferences–>QRGs!

#### Use of two transceivers

When you have configured 2 transceivers in the preferences, the controls will become visible when you widen the logging window. Here you can select the used transceiver, which is indicated by a green dot.
The activated option “Auto toggle” switches a tranceiver active, whenever the frequency changes.

Following restrictions apply:

- Flidgi works with trx #1 only
- microHAM devices work with trx #1 only
- K3/KX3 control window is for trx #1 available only

Reading and writing CW memories within the transceiver and the use of an internal cw-keyer applies to the active trx only, if applicable.

# Subpages

CAT Settings

CW Keyer and CW Memories in Transceiver

K3/KX2/KX3 Control

IC-7300 Control

Options for PTT switching

# External Links

Fldigi

Info Bluetooth Modul