| # DX Cluster Terminal Window

To open the terminal use Menu–>Window–>DX-Cluster Terminal. You can be connected and logged in automatically, when the option Auto log in is set. You can select a dx cluster only, while you are disconnected.
To send a command, type the text and press the Enter key.

When you have set the Auto login option and you open the terminal window:

- The last used dx cluster will be connected.
- You will be logged in with your callsign or user name and password when given.
- The initial commands will be sent.
- When the connection dropps, it is tried to reconnect.

Eight macro buttons are provided at the bottom. Press the Edit button for setup.

In this window you can edit the macros and assign titles to the macro buttons. Placeholders are provided, contents come from the logging fields, or from the last logged QSO:

- <Call>: DX callsign
- <QRG>: Frequency
- <Grid4>: 4-digit grid square
- <Grid6>: 6-digit grid square
- <Manager>:QSL manager

Press a button on the bottom to insert a placeholder into the text, so you don’t need to type it. To send out the command immediately, add <TX>.