## Samsung Tags

Tags found in the binary "STMN" format maker notes written by a number of Samsung models.

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | MakerNoteVersion | undef[8] |
> 2 | PreviewImageStart | int32u* |
> 3 | PreviewImageLength | int32u* |
> 11 | SamsungIFD | - | --> Samsung IFD Tags

## Samsung IFD Tags

This is a standard-format IFD found in the maker notes of some Samsung models, except that the entry count is a 4-byte integer and the offsets are relative to the end of the IFD. Currently, no tags in this IFD are known, so the Unknown (-u) or Verbose (-v) option must be used to see this information.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

## Samsung Type2 Tags

Tags found in the EXIF-format maker notes of newer Samsung models.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | MakerNoteVersion | undef[4] |
> 0x0002 | DeviceType | int32u | 0x1000 = Compact Digital Camera 0x2000 = High-end NX Camera 0x3000 = HXM Video Camera 0x12000 = Cell Phone 0x300000 = SMX Video Camera
> 0x0003 | SamsungModelID | int32u | 0x100101c = NX10 0x1001226 = HMX-S15BP 0x1001233 = HMX-Q10 0x1001234 = HMX-H304 0x100130c = NX100 0x1001327 = NX11 0x170104e = ES70, ES71 / VLUU ES70, ES71 / SL600 0x1701052 = ES73 / VLUU ES73 / SL605 0x1701300 = ES28 / VLUU ES28 0x1701303 = ES74,ES75,ES78 / VLUU ES75,ES78 0x2001046 = PL150 / VLUU PL150 / TL210 / PL151 0x2001311 = PL120,PL121 / VLUU PL120,PL121 0x2001315 = PL170,PL171 / VLUUPL170,PL171 0x200131e = PL210, PL211 / VLUU PL210, PL211 0x2701317 = PL20,PL21 / VLUU PL20,PL21 0x2a0001b = WP10 / VLUU WP10 / AQ100 0x3000000 = WB800F 0x3a00018 = WB2200F 0x400101f = ST1000 / ST1100 / VLUU ST1000 / CL65 0x4001022 = ST550 / VLUU ST550 / TL225 0x4001025 = ST200 / ST200F / ST201 / ST201F / ST205F 0x400103e = VLUU ST5500, ST5500, CL80 0x4001041 = VLUU ST5000, ST5000, TL240 0x4001043 = ST70 / VLUU ST70 / ST71 0x400130a = VLUU ST80, ST80 0x400130e = ST90,ST91 / VLUU ST90,ST91 0x4001313 = VLUU ST95, ST95 0x4a00015 = VLUU ST60 0x4a0135b = ST65 / VLUU ST65 / ST67 0x5000000 = ST700 0x5001038 = WB2000 0x500103a = WB650 / VLUU WB650 / WB660 0x500103c = WB600 / VLUU WB600 / WB610 0x500133e = WB150 / WB150F / WB152 / WB152F / WB151 0x5a0000f = WB5000 / HZ25W 0x6001036 = EX1 0x700131c = VLUU SH100, SH100 0x27127002 = SMX-C20N
> 0x0021 | PictureWizard | int16u | --> Samsung PictureWizard Tags
> 0x0030 | LocalLocationName | string |
> 0x0031 | LocationName | string |
> 0x0035 | PreviewIFD | - | --> Nikon PreviewIFD Tags
> 0x0043 | CameraTemperature | rational64s |
> 0x0045 | RawCompressionMode | int32u |
> 0x0100 | FaceDetect | int16u | 0 = Off 1 = On
> 0x0120 | FaceRecognition | int32u | 0 = Off 1 = On
> 0x0123 | FaceName | string |
> 0xa001 | FirmwareName | string |
> 0xa003 | LensType | int16u[n] | [Value 0] 0 = Built-in or Manual Lens 1 = Samsung NX 30mm F2 Pancake 2 = Samsung NX 18-55mm F3.5-5.6 OIS 3 = Samsung NX 50-200mm F4-5.6 ED OIS 4 = Samsung NX 20-50mm F3.5-5.6 ED 5 = Samsung NX 20mm F2.8 Pancake 6 = Samsung NX 18-200mm F3.5-6.3 ED OIS 7 = Samsung NX 60mm F2.8 Macro ED OIS SSA 8 = Samsung NX 16mm F2.4 Pancake 9 = Samsung NX 85mm F1.4 ED SSA 10 = Samsung NX 45mm F1.8 11 = Samsung NX 45mm F1.8 2D/3D 12 = Samsung NX 12-24mm F4-5.6 ED 13 = Saumsun NX 16-50mm F2-2.8 S ED OIS 14 = Samsung NX 10mm F3.5 Fisheye 15 = Samsung NX 16-50mm F3.5-5.6 Power Zoom ED OIS 20 = Samsung NX 50-150mm F2.8 S ED OIS
> 0xa004 | LensFirmware | string |
> 0xa005 | InternalLensSerialNumber | string |
> 0xa010 | SensorAreas | int32u[8] | (full and valid sensor areas)
> 0xa011 | ColorSpace | int16u | 0 = sRGB 1 = Adobe RGB
> 0xa012 | SmartRange | int16u | 0 = Off 1 = On
> 0xa013 | ExposureCompensation | rational64s |
> 0xa014 | ISO | int32u |
> 0xa018 | ExposureTime | rational64u |
> 0xa019 | FNumber | rational64u |
> 0xa01a | FocalLengthIn35mmFormat | int32u |
> 0xa020 | EncryptionKey | int32u[11]! | (key used to decrypt the tags below)
> 0xa021 | WB_RGGBLevelsUncorrected | int32u[4] | (these tags not corrected for WB_RGGBLevelsBlack)
> 0xa022 | WB_RGGBLevelsAuto | int32u[4] |
> 0xa023 | WB_RGGBLevelsIlluminator1 | int32u[4] |
> 0xa024 | WB_RGGBLevelsIlluminator2 | int32u[4] |
> 0xa028 | WB_RGGBLevelsBlack | int32s[4] |
> 0xa030 | ColorMatrix | int32s[9] |
> 0xa031 | ColorMatrixSRGB | int32s[9] |
> 0xa032 | ColorMatrixAdobeRGB | int32s[9] |
> 0xa033 | CbCrMatrixDefault | int32s[4] |
> 0xa034 | CbCrMatrix | int32s[4] |
> 0xa035 | CbCrGainDefault | int32u[2] |
> 0xa036 | CbCrGain | int32u[2] |
> 0xa040 | ToneCurveSRGBDefault | int32u[23] | (first value gives the number of tone curve entries. This is followed by an array of X coordinates then an array of Y coordinates)
> 0xa041 | ToneCurveAdobeRGBDefault | int32u[23] |
> 0xa042 | ToneCurveSRGB | int32u[23] |
> 0xa043 | ToneCurveAdobeRGB | int32u[23] |
> 0xa048 | RawData? | int32s[12] |
> 0xa050 | Distortion? | int32s[8] |
> 0xa051 | ChromaticAberration? | int16u[22] |
> 0xa052 | Vignetting? | int16u[15] |
> 0xa053 | VignettingCorrection? | int16u[15] |
> 0xa054 | VignettingSetting? | int16u[15] |

## Samsung PictureWizard Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | PictureWizardMode | int16u |
> 0 = Standard 1 = Vivid 2 = Portrait 3 = Landscape 4 = Forest |  | 5 = Retro 6 = Cool 7 = Calm 8 = Classic 9 = Custom1 |  | 10 = Custom2 11 = Custom3 255 = n/a |
> 1 | PictureWizardColor | int16u |
> 2 | PictureWizardSaturation | int16u |
> 3 | PictureWizardSharpness | int16u |
> 4 | PictureWizardContrast | int16u |

## Samsung Trailer Tags

Tags extracted from the trailer of JPEG images written when using certain features (such as "Sound & Shot" or "Shot & More") from Samsung models such as the Galaxy S4 and Tab S.

> Tag Name | Writable | Values / Notes
> --- | --- | ---
> EmbeddedImage | N |
> EmbeddedImageName | N |
> EmbeddedAudioFile | N |
> EmbeddedAudioFileName | N |

## Samsung sec Tags

This information is found in the @sec atom of Samsung MP4 videos from models such as the WB30F.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | N |
> 32 | Model | N |
> 512 | ThumbnailWidth | N |
> 516 | ThumbnailHeight | N |
> 520 | ThumbnailLength | N |
> 524 | ThumbnailImage | N | (the THM image, embedded metadata is extracted as the first sub-document)

## Samsung INFO Tags

This information is found in MP4 videos from Samsung models such as the SMX-C20N.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'EFCT' | Effect | N |
> 'QLTY' | Quality | N |

## Samsung MP4 Tags

This information is found in Samsung MP4 videos from models such as the WP10.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | N |
> 24 | Model | N |
> 46 | ExposureTime | N |
> 50 | FNumber | N |
> 58 | ExposureCompensation | N |
> 106 | ISO | N |
> 125 | Software | N |
> 244 | Thumbnail | - | --> Samsung Thumbnail Tags

## Samsung Thumbnail Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1 | ThumbnailWidth | N |
> 2 | ThumbnailHeight | N |
> 3 | ThumbnailLength | N |
> 4 | ThumbnailOffset | N |

## Samsung smta Tags

This information is found in the smta atom of Samsung MP4 videos from models such as the Galaxy S4.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'svss' | SamsungSvss | - | --> Samsung svss Tags

## Samsung svss Tags

This information is found in the svss atom of Samsung MP4 videos from models such as the Galaxy S4.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Dec 15, 2014

<-- ExifTool Tag Names